Programming PM31

· Unlock Temperature Controller
· Go to Factory page
· Press and hold ADVANCE key (green key with two circular arrows) and infinity (∞) key for six seconds
· CUSt FCty is the first menu choice
· Press ↑until you get to LoC FCty
· [bookmark: _GoBack]Unlocking Temperature Controller
· Press ADVANCE  – LoC.o will appear
· Change value to 0 using ↑↓
· When in the LoC FCty screen, DO NOT change the oFF PAS.E setting as this will lock the controller with a random password
· Press ADVANCE – rLoc5 will appear. Press ↑↓ to get value to 5
· Press ADVANCE – SloC5 will appear. Press ↑↓ to get value to 5
· Press ∞
· Press up arrow until you get to CUSt FCty
· Press ADVANCE and you will see sub-menu 1CUSt
· Press ↑until you get to 3CUSt
· Press ↑↓ to change PAr value to nonE
· Press ∞ to go back to 3CUSt
· Repeat these steps for 3CUSt through 10CUSt (all must have value nonE)
· Press ∞ to return to standard temperature menu
· Hold ↑↓simultaneously until Ai oPEr appears
· Press ↑↓ until LooP oPEr appears
· Press ADVANCE until h.hY (hysteresis) appears. Value should be changed to 5
· Press ∞ to get out of LooP oPEr mode
· Changing High Temperature Limit
· Press ↑↓ simultaneously until Ai Set appears
· Press ↓ until LooP Set appears
· Press Advance key until 130 hsp appears
· Press ↑ until value changes to 160
· Press ∞ twice to return to main screen 
· Locking Temperature Controller 
