Programming SD6
1. Press UP\/DOWN arrow keys simultaneously for 5 seconds

2. SET PAGE appears on display

3. Press BLUE Circular Arrow key to scroll programming parameters
4. Press UP/DOWN arrow keys to change values (upper display in RED)
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To return to the Home screen (bath/set point temperature), press INFINITY key ∞

